**RESCUE 5522**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| |  | | --- | | SERVICE TYPE: Training\_\_\_\_\_Emergency Response\_\_\_\_\_Standby\_\_\_\_\_\_Maintenance\_\_\_\_\_ |   **Name:**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**Date:**\_\_\_\_\_\_\_\_\_\_\_\_\_**Odemeter:**\_\_\_\_\_\_\_\_\_\_\_\_\_**Hrs Spent:**\_\_\_\_\_\_\_\_\_\_(**VEH04 Insp)** | | | |
| **Item** | **Required Status** | **OK** | **Exception Status** |

**CHECK AFTER EACH USE**

|  |  |  |  |
| --- | --- | --- | --- |
| Fuel Level | Minimum ¾ Full (Diesel) |  |  |
| Radio | Response Mode BCFD-S, Default scan ON, Volume level SET |  |  |
| Passenger Window | Closed |  |  |
| Windshield/Mirrors Clean | Inside and Out |  |  |
| Cab Clean | Remove food wrappers/bottles/cans, sweep floor |  |  |
| Accountability Tag | Attached to driver’s door |  |  |
| Map Book | Present, all Topos & reference cards in place |  |  |
| Chassis Lights **\*** | All lights operational. Headlights OFF |  |  |
| Emergency Lights **\*** | All operational |  |  |
| Shore Power | Connected, confirm power ON |  |  |
| Packsets (2+) | Volume SET, Squelch SET, BCFD-S Set |  |  |
| Stream Lights (2) | Turned OFF, confirm charging |  |  |
| Switch Extrication batteries | Tool to charger to tool. **VERIFY TOOLS ARE OFF**. |  |  |
| Accountability Board | Installed in Command compartment, ready for use |  |  |
| Tires **\*** | Visually inspect condition, check pressure by tapping |  |  |
| Tire Chains | If installed, check for tension and condition |  |  |

*\* Remove vehicle from service if any of these items are inoperable and you are unable to repair. Call truck/fleet manager.*

*(see bottom and other side for Monthly or Major Incident Check)*

**COMPLETE MONTHLY OR AFTER MAJOR INCIDENTS *(continue on other side)***

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Required Status** | **OK** | | **Exception Status** |
| *Take radios and streamlights out of chargers, turn on, leave on while completing rest of checklist.*  *Check when done to make sure that the batteries haven’t drained in that amount of time.* | | | | |
| -- Cab -- |  |  |  | |
| Charge Protect | Engages Properly |  |  | |
| Generator controller | Engages Properly |  |  | |
| Garmin GPS | Check batteries-stowed [glove box] |  |  | |
| EMS Response Kit | Restocked, Oxygen refilled and off, all compartments re-sealed [back seat] |  |  | |
| Dash gauges, horn, wipers, heater/def, seatbelts, backup alarm **\*** | Operational |  |  | |
| -- Engine Compartment -- |  |  |  | |
| Engine Oil Level **\*** | 15-30 Multi-Purpose diesel engine oil |  |  | |
| Radiator Fluid Level **\*** | Visible in sight glass |  |  | |
| Power Steering Fluid **\*** | Fill as needed, (ATF) |  |  | |
| Belts and Hoses **\*** | Clean, tight & in good condition |  |  | |
| Engine Batteries | Terminals tight and corrosion free |  |  | |
| -- Outside of Truck -- |  |  |  | |
| Insta-chains | Engage chains, observe proper operation |  |  | |
| SCBA Spare Bottles (4) | Bottles Full and properly stowed |  |  | |
| **5522 -- COMPLETE MONTHLY OR AFTER MAJOR INCIDENTS *(continued from other side)*** | | | | |
| Extinguishers (2) | Gauges showing FULL charge [driver’s rear] |  |  | |
| SCBA Packs (4) | Bottles full, off. Straps extended. Batteries ok. Masks clean. |  |  | |
| -- Extrication Compartment [front compartment] -- | | | | |
| Stabilization struts | Shortened, strap wound, etc [driver’s side] |  |  | |
| Cutter, Spreader, Ram | Tool off, swap batteries to chargers [driver’s side] |  |  | |
| Chain Sets | [passenger’s side] |  |  | |
| Ram Door Supports (2) | [passenger’s side] |  |  | |
| Ram Accessary Kit | [passenger’s side] |  |  | |
| Air Bags & Boards (4) | Clean and stowed properly [passenger side] |  |  | |
| Air Bag Controller | [passenger’s side] |  |  | |
| Air Impact Tools | [passenger’s side] |  |  | |
| Sawzall | Clean, spare blades, battery charged [pass side] |  |  | |
| Cribbing | Stacked neatly [passenger side] |  |  | |
| Hand Tools | Neatly stowed |  |  | |
| Tarps (2) | Clean and stowed [passenger’s side] |  |  | |
| -- Traffic /Rescue Compartment [middle] -- | | | | |
| Stokes Liter | Clean & properly stowed on top |  |  | |
| Scoops (1) | Clean & properly stowed with all straps secured |  |  | |
| Backboards (4) | Boards and straps clean and properly secured |  |  | |
| Traffic control signs (2) | Clean & properly stowed in middle compartment |  |  | |
| Traffic Accident signs (2) | Clean & properly stowed in middle compartment |  |  | |
| Traffic cones | Clean & properly stowed in first compartment |  |  | |
| Snacks | Restocked [middle compartment] |  |  | |
| Water & Gator Aid | Restocked [middle compartment] |  |  | |
| Blankets | Restocked [middle compartment] |  |  | |
| Ropes Kit | Restocked [middle compartment] |  |  | |
| Electric Cord Reel | Properly rewound |  |  | |
| Light Tower | Raises & lowers, all lights work, requires generator to be engaged |  |  | |
| Emergency Triangles | Clean and properly stowed |  |  | |
| -- Medical Compartment [passenger rear side] -- | | | | |
| Pediatric kit | Stocked, all compartments closed |  |  | |
| Portable Oxygen (3) | Refilled, properly stowed (1 Med bag, 2 spare) |  |  | |
| Defibrillator | Clean, stowed, battery level okay |  |  | |
| Pulse Oximeter | Clean, stowed, batter level okay |  |  | |
| Suction | Clean, stowed, plugged in |  |  | |
| -- Command Compartment -- | | | | |
| Blank forms | Call, Training &Activity Report forms |  |  | |
| Writing Tools | Pens, Grease Pencils, White Board Markers, etc. |  |  | |
| MAPS | USGS Maps, County Maps, District Maps |  |  | |
| General Office Materials | Stick pins, Post-it Notes, Paper, Paper clips , etc. |  |  | |
| IC compartment clipboards | Vest(s), pen/pencil, paper, forms |  |  | |
| Binoculars | Clean & properly stowed |  |  | |
| Spare Batteries | A stock of AA, 9 volt, & C batteries |  |  | |
|  |  |  |  | |
| Keep reasonably clean | Pressure wash, including underside of truck |  |  | |
| *Verify streamlights and radios still working. Turn off, place in chargers, verify charging.* | | | | |

*\* Remove vehicle from service if any of these items are inoperable and you are unable to repair. Call truck/fleet manager.*