**5544**

|  |
| --- |
| SERVICE TYPE: Training\_\_\_\_\_Emergency Response\_\_\_\_\_Standby\_\_\_\_\_\_Maintenance\_\_\_\_\_ |

**Name:**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**Date:**\_\_\_\_\_\_\_**Odemeter:**\_\_\_\_\_\_\_\_\_Duration**:**\_\_\_\_\_\_\_\_**VEH04 Inspection**

|  |  |  |  |
| --- | --- | --- | --- |
| Revised 3-2-2016 | **Required Status** | **OK** | **Exception Status** |
| **COMPLETE MONTHLY OR AFTER MAJOR INCIDENT** | | | |
| Engine Oil Level | 15-30 Multi-Purpose Oil |  |  |
| Radiator Fluid Level | Visible in Overflow tank |  |  |
| Power Steering Fluid | Fill as needed (ATF) |  |  |
| Windshield Washer Fluid | Fill as needed |  |  |
| Belts and Hoses | Clean, tight and in good condition |  |  |
| Batteries (annually) | Under passenger seat Terminals clean and tight |  |  |
| DEF | Add if less than ½ full |  |  |
| Bleed Air Tanks | Bleed water out |  |  |
| Pump-to-Tank Valve | Hold button a couple of seconds after light comes on to assure valve is closed |  |  |
| Drain Valves | Operate drain valves-Leave closed. In cold weather drain and leave drains open |  |  |
| Pump Panel | Discharges closed |  |  |
| Extinguishers (2) | Gauges showing FULL charge |  |  |
| Hard Suction (3) | Gaskets clean and in place, stowed |  |  |
| Hoses and Nozzles | Clean and properly stowed |  |  |
| Fittings & Adapters | All fittings clean, stowed, ready for use |  |  |
| Water Nozzles | Clean & properly stowed |  |  |
| Port-a-Pond | Clean and stowed properly, Open side up |  |  |
| Quick dump chutes (3) | While outside, activate quickly to assure operation |  |  |
| 2 ½” & LDH Hydrant valves | Clean, gaskets in place, valve closed, stowed |  |  |
| 2 ½” & LDH fill hoses | Clean, Gaskets in place, stowed |  |  |
| Misc. tools | Properly stowed |  |  |
| Check for Fault Conditions | Rotate Menu Control Switch to Diagnostic Display  If Fault indicated, Identify and notify Fleet Manger |  |  |
| Drive truck | Activate auto chains. Check for proper operation  Observe & record any odd noises. Observe proper operation |  |  |
| Exhaust Particle Filter | Less than ¾ full—Make arrangements to clean |  |  |
| Drive and operate truck \* | Check feel of steering, brakes, shifting, suspension.\*  Run pump, circulate water, build 100 psi pressure.  Momentarily operate each quick-dump.  Check operation of automatic chains.  Observe & record any odd noises, vibrations, smells, leaks, etc.  Check parking brake holds both up- and downhill. |  |  |
| *>> Verify streamlight and radio batteries not discharged, return to chargers, verify charging.* | | | |

*\* Remove vehicle from service if any of these items are inoperable and you are unable to fix. Call truck/fleet manager.*

**5544**

|  |
| --- |
| **SERVICE TYPE: Training\_\_\_\_\_Emergency Response\_\_\_\_\_Standby\_\_\_\_\_\_Maintenance\_\_\_\_\_** |

**Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Date:\_\_\_\_\_\_\_Odemeter:\_\_\_\_\_\_\_\_\_Hours:\_\_\_\_\_\_\_\_VEH04 Inspection**

|  |  |  |  |
| --- | --- | --- | --- |
| Revised 3-2-2016 | **Required Status** | **OK** | **Exception Status** |

**CHECK AFTER EACH APPARATUS USE**

|  |  |  |  |
| --- | --- | --- | --- |
| Fuel Level | Minimum ¾ full (Diesel) |  |  |
| Radio | Response Mode-BCFD-S, default Scan-ON, Volume SET |  |  |
| Packset (1) | Volume SET, Squelch OFF, BCFD-S selected |  |  |
| Stream Lights (2) | Turned OFF, confirm charging |  |  |
| Passenger Window | Closed |  |  |
| Pump PTO control | Disengaged |  |  |
| Windshield Clean | INSIDE and OUT |  |  |
| Mirrors set properly | Left & Right |  |  |
| Accountability tag | Attached to driver’s door |  |  |
| Map Book | Present, all topos & reference cards in place |  |  |
| Front Axle Lock | OFF |  |  |
| Differential Lock | OFF |  |  |
| DEF Regen Switch | Neutral Position (DO NOT select OFF or START w/o instructions |  |  |
| ENG Jake Brake | OFF |  |  |
| Off Road ABS | OFF |  |  |
| Automatic Chains | OFF |  |  |
| Water Tank Level | All lights ON |  |  |
| Foam Tank Level | ¾ + full |  |  |
| Chassis Lights | All lights operational, Headlight switches OFF |  |  |
| Emergency Lights | All lights operational, Emergency Master OFF |  |  |
| Master Switch | Off, After 1 Minute Delay |  |  |
| Shore Power | Connected, Confirm power ON |  |  |
| Tires | Visually check condition |  |  |
| Wheel Chocks | Clean and in racks |  |  |
| Tire Chains | Installed-Tension & Condition- or properly stowed |  |  |
| Compartment Doors | CLOSED |  |  |
| Hose/Hydrant Wrenches | All in place |  |  |
| In COLD weather | Open all drains. Remove, drain and replace inlet and outlet covers. Blow out Reel |  |  |
|  |  |  |  |
|  |  |  |  |
| (see other side for Monthly or Major Incident Check)  **TENDER 5544** | | | |