**5503**

|  |
| --- |
| **SERVICE TYPE****: [ ] Training** **[ ] Emergency [ ] Response [ ] Standby [ ] Maintenance** |

**Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Date:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Odemeter:\_\_\_\_\_\_\_\_\_\_\_Hours Spent:\_\_\_\_\_\_\_\_****VEH04 Insp.**

**CHECK AFTER EACH USE**

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Item** | **Spec** | **Notes** |
|  | Fuel Level | Minimum ¾ Full |  |
|  | Pump PTO Control | Disengaged |  |
|  | Compressor Control | OFF-Switch on Pump Panel |  |
|  | Radio | Response Mode BCFD-S default, Scan ON Volume level SET |  |
|  | Packsets (2) | Volume & Squelch OFF, BCFD-S Selected |  |
|  | Passenger Window | Closed |  |
|  | Windshield/Mirror Glass | Clean both inside & out |  |
|  | Mirrors set properly | Right and left |  |
|  | Cab Clean | Remove wrappers/bottles/cans, sweep floor |  |
|  | Front Axle Lock | OFF |  |
|  | Map Book | Present, all topos & ref cards in place |  |
|  | Accountability Tag | Attached to driver’s door |  |
|  | Chassis Lights | All lights operating, Head lights OFF |  |
|  | Emergency Lights | All lights operating, Master Switch OFF |  |
|  | Water Tank Level | 4 lights ON |  |
|  | Master Switch | OFF |  |
|  | Shore Power | Connected-Confirm charging |  |
|  | Stream Lights (2) | Turned OFF, confirm charging |  |
|  | Tires | Visually inspect for damage, Test for pressure by Tapping, Check for rocks stuck between rear duals |  |
|  | Wheel Chocks | Clean and stowed |  |
|  | Tire Chains | If installed-tension and condition or properly stowed |  |
|  | Compartment Doors | Closed |  |
|  | Inlet & Outlet Covers | All caps on |  |
|  | Hose/Hydrant Wrenches | All are in place |  |

**Truck Manager:** Chad Hamre, 720.713.9596
**Doc Updated:** 2021-08-25

**5503**

|  |  |
| --- | --- |
| **SERVICE TYPE: [ ] Training [ ] Emergency [ ] Response [ ] Standby [ ] Maintenance** |  |

**Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Date:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Odemeter:\_\_\_\_\_\_\_\_\_\_\_Hours Spent:\_\_\_\_\_\_\_\_VEH04 Insp.**

**CHECK MONTHLY AND AFTER MAJOR INCIDENTS**

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Item** | **Spec** | **Notes** |
|  | Engine Oil Level | 15-30 Multi-Purpose diesel engine oil |  |
|  | Radiator fluid Level  | Level within 3 inches of top of radiator |  |
|  | Belts | Clean, tight and in good condition |  |
|  | Batteries | Terminals tight & corrosion free |  |
|  | Foam Tank Level | Full |  |
|  | Drain valves | Operate valves-Leave drained & closed |  |
|  | Air Tanks | Bleed any accumulated water from tanks |  |
|  | Pump Panel | Discharges closed, CAFS system OFF, Air valves closed |  |
|  | Primer Pump Oil  | Reservoir at least 80% full |  |
|  | Auto Transmission Fluid | Within range |  |
|  | Power Steering Fluid | Within range |  |
|  | Air Compressor Oil | Within range |  |
|  | Port-a-Pond | Clean & stowed with ropes on top |  |
|  | Ladders (2) | Clean & stowed |  |
|  | Hard Suction (2) | Clean & stowed-Gaskets in place |  |
|  | Pike Pole | Clean & stowed |  |
|  | Cross-lay Hose & Nozzles | Properly flaked, CAFS nozzle installed & closed |  |
|  | Fittings & adapters | Clean, stowed & ready for use |  |
|  | SCBA packs (4) | Bottles full & off -straps extended -Masks clean |  |
|  | SCBA Spare Bottles (4) | Full & OFF, straps extended, batteries okay. |  |
|  | Gas Detector | Recharged, clean, spare batteries & screwdriver |  |
|  | EMS Response Kit | Restocked, Oxygen refilled, all compartments resealed |  |
|  | Defibrillator | Clean, stowed, spare battery on charge |  |
|  | Pulse Oximeter | Clean and properly stowed |  |
|  | Portable suction | Clean, restocked, stowed & on charge |  |
|  | Back Boards | Clean, properly secured, C-Collars & head pads in med compartment |  |
|  | Traffic Control Signs | Two signs, clean and stowed |  |
|  | Backpack pumps (3) | Clean, empty, ready for use |  |
|  | Wildfire hand tools | Clean and stowed properly |  |
|  | Extinguishers (2) | Gauges show fully charged |  |
|  | Axes (large & small) | Clean and stowed |  |
|  | Bolt Cutter | Clean, adjusted and stowed |  |
|  | Operate all Valves | Check for free operation |  |
|  | Tires | Ensure tire pressure is at max pressure on sidewall. |  |
|  | In cold weather | Remove, drain & replace all inlet & outlet covers. Drain pump & plumbing. Chains on and tight if appropriate.  |  |
|  | Operate truck | [ ] Check the feel of steering, brakes, shifting, suspension. [ ] Run pump, circulate water, build 100 psi pressure.[ ] Verify parking brake holds on steep up- and downhill.[ ] Observe & record any odd noises, vibrations, smells, leaks, etc.  |  |
|  | Keep reasonably clean | Pressure wash if necessary, including underside of truck |  |