|  |
| --- |
| **SERVICE TYPE: Training\_\_\_\_\_Emergency Response\_\_\_\_\_Standby\_\_\_\_\_\_Maintenance\_\_\_\_\_** |

**5541 / 5542**

**Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Date:\_\_\_\_\_\_\_Odometer:\_\_\_\_\_\_\_\_\_Hours Spent:\_\_\_\_\_\_ [VEH04 Insp]**

|  |  |  |  |
| --- | --- | --- | --- |
| **CHECK AFTER EACH USE** | | | |
|  | **Required Status** | **OK** | **Action Req’d** |
| Fuel Level | Minimum ¾ full (Diesel) |  |  |
| Radio | Response Mode-BCFD-S, Scan-ON, Volume OK |  |  |
| Packset (1) | Squelch OFF, BCF-S selected, Radio OFF, charging |  |  |
| Stream Lights (2) | Turned OFF, confirm charging |  |  |
| Passenger Window | Closed |  |  |
| Pump PTO control | Disengaged |  |  |
| Windshield Clean | INSIDE and OUT |  |  |
| Mirrors set properly | Left & Right |  |  |
| Accountability tag | Attached to driver’s door |  |  |
| Map Book | Present, all topos & reference cards in place |  |  |
| Front Axle Lock | OFF |  |  |
| Differential Lock | OFF |  |  |
| Automatic Chains | OFF |  |  |
| Water Tank Full | All lights ON |  |  |
| Chassis Lights \* | All lights operational (including under-body lights). Headlight switch on halfway (parking lights on, headlights off) |  |  |
| Emergency Lights | All lights operational/on, Emergency Master OFF |  |  |
| Master Switch | Off |  |  |
| Shore Power | Connected, Confirm power ON |  |  |
| Tires | Visually check condition, check duels for rocks. |  |  |
| Wheel Chocks | Clean and in racks |  |  |
| Tire Chains | Installed-Tension & Condition- or properly stowed |  |  |
| Compartment Doors | Closed |  |  |
| Hose/Hydrant Wrenches | All in place |  |  |
| In FREEZING weather | Open all drains. Remove, drain, dry and replace inlet and outlet covers. Blow out Reel with air. |  |  |
|  |  |  |  |
|  |  |  |  |
| (see other side for Monthly or Major Incident Check) | | | |

5541 manager: Heather Winner

5542 manager: Sandra Bailey

|  |
| --- |
| SERVICE TYPE: Training\_\_\_\_\_Emergency Response\_\_\_\_\_Standby\_\_\_\_\_\_Maintenance\_\_\_\_\_ |
|  |

**Name:**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**Date:**\_\_\_\_\_\_\_**Odometer:**\_\_\_\_\_\_\_\_\_**Hours Spent:**\_\_\_\_\_ **[VEH04 Insp]**

**5541 / 5542**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **CHECK MONTHLY OR AFTER MAJOR INCIDENT** | | | | |
|  | | **Required Status** | **OK** | **Action Req’d** |
| *>> Remove radios and streamlights from chargers, turn on for duration of monthly check* | | | | |
| IN CAB | Dash gauges/lights, horn, wipers, heater/def, seatbelts, backup alarm **\*** | All operational |  |  |
| SCBA 02 (5541 only) | Should be full |  |  |
| Backup camera | Operational |  |  |
| Map book | Present, organized |  |  |
| UNDER HOOD | Engine Oil Level \* | 15-30 Multi-Purpose Diesel Engine Oil |  |  |
| Transmission Fluid Levl \* |  |  |  |
| Radiator Fluid Level \* | Visible in Overflow tank |  |  |
| Power Steering Fluid \* | Fill as needed (ATF) |  |  |
| Windshield Washer Fluid | Fill as needed |  |  |
| Belts and Hoses \* | Clean, tight and in good condition |  |  |
| PASS SIDE | Batteries | Terminals clean and tight |  |  |
| Extinguishers (2) | Both gauges showing FULL charge |  |  |
| Warning triangles | Present and in serviceable condition |  |  |
| Primer Fluid (5542 only) | Full of environmentally-friendly antifreeze in passenger side Access Door |  |  |
| Port-a-Pond | Clean and stowed properly, Open side up |  |  |
| REAR | Hard Suction (3) | Gaskets clean and in place, secured in place |  |  |
| Quick dump chutes (3) | Free of damage, debris, etc |  |  |
| Bleed Air Tanks | Pull cables under rear bumper, bleed until no water remains |  |  |
| PUMP PL | All valves closed | For electric valves, hold button 1+ second after light comes on to assure valves are closed |  |  |
| Drain Valves | Operate drain valves to flush dirt. Leave closed in summer, open in winter |  |  |
| DRIVERS SIDE | Fittings & Adapters | All fittings clean, stowed, ready for use |  |  |
| 1½” Hoses and Nozzles | Clean and properly stowed |  |  |
| 2 ½” & 4” hydrant valves | Clean, gaskets in place, valve closed, stowed |  |  |
| 2 ½” & LDH fill hose | Clean, Gaskets in place, stowed |  |  |
| Misc. tools in upper rack | Properly stowed |  |  |
| Drive and operate truck \* | | Check feel of steering, brakes, shifting, suspension.\*  Run pump, circulate water, build 100 psi pressure.  Momentarily operate each quick-dump.  Check operation of automatic chains.  Observe & record any odd noises, vibrations, smells, leaks, etc.  Check parking brake hold both up- and downhill. |  |  |
| *>> Verify streamlight and radio batteries not discharged, return to chargers, verify charging.* | | | | |

*\* Remove vehicle from service if any of these items are inoperable and you are unable to fix. Call truck/fleet manager.*